# Summary

The Summary section of the HTML report contains several tables summarizing the fitting results for your design.
The Header table contains the following:

- The Design Name
- The Fitting Status, which is one of the following:

- Successful
- Design Rule Checking Failed
- Placement Failed
- Routing Failed

- The Software Version
- The Device Used, with a link to a PDF version of the device documentation
- The Date and time of completion

The Resources Summary table includes:

- The number and percentage of macrocells used vs total in device
- The number and percentage of product terms used vs total in device
- The number and percentage of registers used vs total in device
- The number and percentage of pins used vs total in device
- The number and percentage of function block inputs used vs total in device

The Pin Resources table includes two tables:

- The first table indicates the requirements of the design, broken up by Signal Type. The number required and the number mapped onto the device are indicated for each signal type.
- The second table gives the total number of each pin type available in the device, alongwith the number used.

XPLA3 only - The Local Control Term Resources table lists the local control term mapping for each function block:

- Each row lists the local control term mapping for each of the eight control terms, LCT0-LCT7, in a function block.
- The control term mapping can be:

- ce - clock enable
- clk - clock
- ee - output enable
- sr - set/reset
- uct1 - universal control term clock
- uct2 - universal control term output enable
- uct3 - universal control term set
- uct4 - universal control term reset

- Each LCT can have some subset of the signals above mapped onto them:

- LCT0 - sr, oe
- LCT1 - sr, oe
- LCT2 - sr, oe
- LCT3 - sr
- LCT4 - ce, clk, sr
- LCT5 - clk, sr
- LCT6 - clk, oe
- LCT7 - clk, uct1/uct2/uct3/uct4

The Global Resources table indicates the signals used as global signals in the device.

XC9500/XL/XV only - The Power Data table indicates the number of macrocells in standard and low power mode.

XPLA3 only - The Block Resources table indicates the number of function block control terms used vs available and the number of foldback NANDs used vs available.