### Summary

Design Name | MegaSpeedy
Fitting Status | Successful
Software Version | P.20131013
Device Used | XC95144XL-10-TQ100
Date | 3-27-2015, 11:23PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
131/144 (91%) | 478/720 (67%) | 56/144 (39%) | 81/81 (100%) | 348/432 (81%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 28 | 28
Output | 41 | 41
Bidirectional | 11 | 11
GCK | 1 | 1
GTS | 0 | 0
GSR | 0 | 0
Pin Type | Used | Total
--- | --- | ---
I/O | 73 | 74
GCK/IO | 3 | 3
GTS/IO | 4 | 4
GSR/IO | 1 | 1

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK3) | phi2

##### POWER DATA

Macrocells in high performance mode (MCHP) | 0
Macrocells in low power mode (MCLP) | 131
Total macrocells used (MC) | 131