# Pin List

The Pin List page lists each pin of your design with its pin type and associated signal. Check boxes at the top of the table allow you to select and deselect which pin types you want displayed in the table (the default view will display all of them).

Note: There is a
button below the table. Click this button to open a new window describing all of the acronyms used in the function block table. You can select either brief descriptions or more detailed descriptions by clicking the "Verbose" button at the top of the window.

Clicking on the underscored pin numbers in the first column of the table will open a new window displaying the pin layout diagram for the selected pin. Rolling your mouse over the colored pin will pop up a tooltip with the signal name assigned to the pin, the I/O standard, the I/O style, the slew rate, and/or any constraints assigned to the pin:

Clicking any underscored signal in the third column of the table will open a new window displaying the equations for that particular signal.

Clicking on the
button at the top of the screen will open a new window with a graphical, top view of all of the pins:

They are color-coded as follows:

Color | Signal
Green | Input
Aqua | Bidirectional
Blue | Output
Magenta | Clock
Red | VCC
Black | GND
Yellow | TDO
Gray | TDI
White | Unused Pin
Black Outline | No available Pad

As with the single pin display, rolling your mouse over any colored pin will pop up a tooltip with the signal name assigned to the pin, the I/O standard, the I/O style, the slew rate, and/or any constraints assigned to the pin.